!
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
!
!
!
no ip icmp rate-limit unreachable
!
!         
!
!
hostname
!
ip cef
no ip domain-lookup
!
!
ip tcp synwait-time 5
!
!
!
!
interface Ethernet0/0
 no ip address
 no shutdown
!
interface Ethernet0/1
 no ip address
 no shutdown
!
interface Ethernet0/2
 no ip address
 no shutdown 
!
interface Ethernet0/3
 no ip address
 no shutdown
!
interface Ethernet1/0
 no ip address
 no shutdown
!
interface Ethernet1/1
 no ip address
 no shutdown
!
interface Ethernet1/2
 no ip address
 no shutdown
!
interface Ethernet1/3
 no ip address
 no shutdown
!
interface Serial2/0
 no ip address
 no shutdown
 serial restart-delay 0
!
interface Serial2/1
 no ip address
 no shutdown
 serial restart-delay 0
!
interface Serial2/2
 no ip address
 no shutdown
 serial restart-delay 0
!
interface Serial2/3
 no ip address
 no shutdown
 serial restart-delay 0
!
interface Serial3/0
 no ip address
 no shutdown
 serial restart-delay 0
!         
interface Serial3/1
 no ip address
 no shutdown
 serial restart-delay 0
!
interface Serial3/2
 no ip address
 no shutdown
 serial restart-delay 0
!
interface Serial3/3
 no ip address
 no shutdown
 serial restart-delay 0
!
!
no cdp log mismatch duplex
!
line con 0
 exec-timeout 0 0
 privilege level 15
 logging synchronous
line aux 0
 exec-timeout 0 0
 privilege level 15
 logging synchronous
!
end
